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Flying with Your Omni Wheelchair – Lithium-Ion Battery Guidelines
Your Omni wheelchair is equipped with a non-removable lithium-ion battery system which meets the requirements of the tests laid out by standard UN38.3.
To ensure your wheelchair can travel safely by air, please follow the instructions below.
1. Battery Specification
Chemistry:	Lithium-Ion (Li-ion)
Voltage:	48 VDC
Capacity:	44 Ah (2,112 Wh)

	Note: advance airline approval is required, check airline policy carefully.



2. Pre-Flight Preparation
· Isolate the battery as described in the Omni User Manual and in this document.  
The battery is non-removable.  All terminals are insulated to protect from short circuits.
· Prepare Documentation
Provide the airline with:
1. Manufacturer’s battery guidance sheet (this document).
1. Battery specification (Lithium-Ion, 48 V, 44 Ah, 2112 Wh).
1. Statement that the battery has been isolated.

3. Airline Notification
· Follow airline instructions for large lithium-ion battery transport 
· Always notify the airline well in advance (usually at booking and again at check-in).
· Provide:
· Battery type, voltage, and Wh rating.
· Confirmation that it has been isolated and terminals insulated.
· Any additional airline-specific forms as required.


4. During Travel
· The wheelchair can be checked in once the battery is isolated.
· Do not attempt to reconnect the battery on board.
· Follow airline staff instructions regarding storage and handling of your wheelchair and battery.

5. Reconnecting After Flight
1. After arrival, inspect the wheelchair for damage.
2. Reconnect battery as described in the Omni User Manual and in this document.

References:
· IATA Dangerous Goods Regulations
https://www.iata.org/en/programs/cargo/dgr/
· Lithium Battery Guidance for Air Transport 
Lithium batteries that are used to power the wheelchairs and mobility aids must be of a type which meets the requirements of each test in the UN Manual of Tests and Criteria, Part III, subsection 38.3. 
The lithium battery(ies) can either remain installed in the wheelchair or mobility aid, if the battery(ies) is protected against damage by the design and securely attached or be removed, following the manufacturer’s instructions.  ).
While there is no regulatory limit to the Watt-hour (Wh) rating if the battery(ies) remain installed; operators are still subject to the provisions of DGR 9.1.9 (Requirement for Safety Risk Assessment) and DGR 1.4.2.2 (Recommendations with respect to approval of dangerous goods carried by passengers and crew). Further guidance can be found in the IATA document “Lithium Battery Risk Assessment Guidance for Operators”
https://www.iata.org/contentassets/6fea26dd84d24b26a7a1fd5788561d6e/mobility-aid-guidance-document.pdf
· [image: A qr code on a white background

Description automatically generated]UN38.3 Certificate of Testing for the Omni wheelchair batteries
https://www.conqueringhorizons.com/
For certificates and an electronic copy of this document,
please scan the QR code.
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ISOLATE THE BATTERY
In accordance with the Omni User Manual isolate the battery to remove all power from the device
“The device is isolated when the indicator flag is pointing downwards as shown below.  To isolate the device, depress the red button; to re-connect the device, lift the flag up to the horizontal position.”

OMNI WHEELCHAIR – AIR TRAVEL

LITHIUM-ION BATTERY ISOLATION GUIDELINES
BATTERY DATA
48V 44Ah (2112Wh) LITHIUM-ION SYSTEM
(NON-REMOVABLE)
NOTIFY AIRLINE
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